DG2000 Series Function/Arbitrary Waveform Generator Programming Guide

This manual is for users who want to use remote commands to control RIGOL DG 2 000 Series Function/Arbitrary Waveform Generator. We assume that readers of this manual have read User¡¯s Guide for RIGOL DG2000 Series and gotten familiar with the usage of the generator.

¡¡

DG 2 000 Series instrument can communicate with the PC through USB, LAN, GPIB and RS232 instrument buses. For the usage of each communication method, please refer to the User¡¯s Guide of this instrument. Users can use the command programming to control the instrument, after the DG 2 000 Series instrument is reliably connected with the PC via one of the above-mentioned methods. All the command words are transimmited to the instrument from the PC and identified as ASCII string to realize operation, control and secondary development of the instrument.

The following operations can be realized through programming:

¡¡

¡ñ Set up the signal generator.

¡ñ Output waveform data from the signal generator.

¡¡

¡¡

¡¡

¡¡

Introduction to the SCPI Language

Command System

Programming Examples

Command Qucik Reference A-Z

Contact Us

© 2010 RIGOL Technologies, Inc. All Rights Reserved.

¡¡

¡¡