FUNCtion:SQUare:DCYCle

¡¡

¡¡

Syntax

¡¡

FUNCtion:SQUare:DCYCle {<percent>|MINimum|MAXimum}
FUNCtion:SQUare:DCYCle? [MINimum|MAXimum]

¡¡

¡¡

Description

¡¡

Set or query the duty cycle for square waves.

¡¡

¡¡

Explanation

¡¡

<percent> is the duty cycle percentage selected by the user, MIN is the minimum duty cycle of the selected frequency and MAX is the maximum duty cycle of the selected frequency.

Different frequency ranges correspond to different upper and lower limits of duty cycle:
¡Ü 8MHz: 20% to 80%
8MHz to 16MHz: 40% to 60%
>16MHz: 50%

¡¡

¡¡

Return Value

¡¡

FUNC:SQU:DCYC? returns the current duty cycle.

FUNC:SQU:DCYC? M AX always returns the maximum duty cycle.

FUNC:SQU:DCYC? MIN always returns the minimum duty cycle.

¡¡

¡¡

Example

¡¡

Set the duty cycle to 60%: FUNC:SQU:DCYC 60

Return Value: 60.000000

¡¡

¡¡

Related Commands

¡¡

APPLy:SQUare

¡¡

¡¡

¡¡