BURSt:MODE

¡¡

¡¡

Syntax

¡¡

BURSt:MODE {TRIGgered|GATed}
BURSt:MODE?

¡¡

¡¡

Description

¡¡

Select the burst mode and the default burst mode is TRIGgered.

¡¡

¡¡

Explanation

¡¡

TRIGgered: trigger mode. In trigger mode, the generator outputs a waveform with specified number of cycles (using the BURSt:NCYCles command) each time a trigger is received from the specified trigger source (using the TRIGger:SOURce command).

GATed: gated mode. T he output waveform is either "ON" or "OFF" based on the level of the external signal applied to the [Ext Trig/FSK/Burst] connector at the rear panel.

¡¡

¡¡

Return Value

¡¡

The query returns TRIG or GAT.

¡¡

¡¡

Example

¡¡

Select the gated mode as the burst mode: BURS:MODE GAT

Return Value: GAT

¡¡

¡¡

¡¡

¡¡