FREQuency:STARt

¡¡

¡¡

Syntax

¡¡

FREQuency:STARt {<frequency>|MINimum|MAXimum}
FREQuency:STARt? [MINimum|MAXimum]

¡¡

¡¡

Description

Set the start frequency (used in conjunction with the stop frequency) in the Sweep mode and the default unit is Hz.

¡¡

Explanation

¡¡

<frequency> is the frequency value set by the user, MIN selects the minimum start frequency allowed by the specific function and MAX selects the maximum start frequency allowed by the specific function.

¡¡

¡¡

Return Value

¡¡

FREQuency:STARt? returns the current start frequency.

FREQuency:STARt? M AX always returns the maximum value of the start frequency.

FREQuency:STARt? MIN always returns the minimum value of the start frequency.

¡¡

¡¡

Example

¡¡

Set the start frequency to 1kHz: FREQ:STAR 1000

Return Value: 1.000000e+03

¡¡

¡¡

Related Commands

¡¡

FREQuency:STOP

¡¡

¡¡

¡¡