FREQuency:CENTer

¡¡

¡¡

Syntax

¡¡

FREQuency:CENTer {<frequency>|MINimum|MAXimum}
FREQuency:CENTer? [MINimum|MAXimum]

¡¡

¡¡

Description

Set the center frequency (used in conjunction with the frequency span) in Sweep mode and the default unit is Hz.

¡¡

Explanation

¡¡

<frequency> is the frequency value set by the user, MIN selects the minimum center frequency allowed by the specific function and MAX selects the maximum frequency allowed by the specific function.

¡¡

¡¡

Return Value

¡¡

FREQuency:CENTer? returns the current center frequency.

FREQuency:CENTer? M AX always returns the maximum value of the center frequency.

FREQuency:CENTer? MIN always returns the minimum value of the center frequency.

¡¡

¡¡

Example

¡¡

Set the center frequency to 550Hz: FREQ:CENT 550

Return Value: 5.500000e+02

¡¡

¡¡

Related Command

¡¡

FREQuency:SPAN

¡¡

¡¡