FSKey:INTernal:RATE

¡¡

¡¡

Syntax

¡¡

FSKey:INTernal:RATE {<rate in Hz>|MINimum|MAXimum}
FSKey:INTernal:RATE? [MINimum|MAXimum]

¡¡

¡¡

Description

¡¡

Set the rate at which the output frequency "shifts" between the carrier and hop frequency and the unit is Hz.

¡¡

¡¡

Explanation

¡¡

<rate in Hz> is the frequency value set by the user, MIN is the minimum value of the FSKey frequency and MAX is the maximum value of the FSKey frequency.

Select the carrier waveform frequency using the FREQuency command.

Select the hop frequency using the FSKey:FREQuency command.

¡¡

¡¡

Return Value

¡¡

FSKey:INTernal:RATE? returns the current FSKey frequency.

FSKey:INTernal:RATE? MAX always returns the maximum value of the FSKey frequency.

FSKey:INTernal:RATE? MIN always returns the minimum value of the FSkey frequency.

¡¡

¡¡

Example

¡¡

Set the FSkey frequency to 100Hz: FSK:INT:RATE 100

Return Value: 1.000000e+02

¡¡

¡¡

¡¡

¡¡