PM:INTernal:FREQuency

¡¡

¡¡

Syntax

¡¡

PM:INTernal:FREQuency {<frequency>|MINimum|MAXimum}
PM:INTernal:FREQuency? [MINimum|MAXimum]

¡¡

¡¡

Description

Set the frequency of the modulating waveform when the internal modulation source is selected and the unit is Hz.

¡¡

Explanation

¡¡

<frequency> is the frequency value set by the user, MIN is the minimum frequency of the current modulating waveform and MAX is the maximum frequency of the current modulating waveform.

To select internal modulation, refer to the PM:SOURce command.

To set the carrier waveform frequency, use the FREQuency command.

¡¡

¡¡

Return Value

¡¡

PM:INTernal:FREQuency? returns the frequency of the current internal modulating waveform.

PM:INTernal:FREQuency? MAX always returns the maximum frequency of the current internal modulating waveform.

PM:INTernal:FREQuency? MIN always returns the minimum frequency of the current internal modulating waveform.

¡¡

¡¡

Example

¡¡

Set the frequency of the internal modulating waveform to 100Hz: PM:INT:FREQ 100

Return Value: 1.000000e+02

¡¡

¡¡

Related Commands

¡¡

PM:SOURce

FREQuency

¡¡

¡¡

¡¡

¡¡