FREQuency

¡¡

¡¡

Syntax

¡¡

FREQuency {<frequency>|MINimum|MAXimum}
FREQuency? [MINimum|MAXimum]

¡¡

¡¡

Description

¡¡

This command sets the output frequency of the basic waveform (SINusoid|SQUare|RAMP|PULSe|NOISe|USER) and the default unit is Hz.

¡¡

¡¡

Explanation

¡¡

<frequency> is the frequency value set by the user, MIN selects the lowest frequency allowed by the selected function and MAX selects the highest frequency allowed.

¡¡

¡¡

Return Value

¡¡

FREQuency? returns the current output frequency.

FREQuency? M AX always returns the maximum value of the output frequency allowed.

FREQuency? MIN always returns the minimum value of the output frequency allowed.

¡¡

¡¡

Example

¡¡

Set the output frequency to 1kHz: FREQ 1000

Return Value: 1.000000e+03

¡¡

¡¡

¡¡

¡¡