APPLy:DC

¡¡

¡¡

Syntax

¡¡

APPLy:DC [<frequency>[,<amplitude>[,<offset>]]]

¡¡

¡¡

Description

¡¡

This command is used for generating a DC voltage with the level specified by the offset.

¡¡

¡¡

Explanation

¡¡

The <frequency> and <amplitude> parameters have no effect for this command and are substituted to "0" when using this command.
If you specify a frequency and amplitude, they have no effect for the DC output, but the values are remembered when you switch to another function.

If no parameter is set, the system will output according to the current parameter and unit.

¡¡

¡¡

Example

¡¡

Output a DC voltage with the offset as -1.5Vdc:

APPL:DC 0,0,-1.5

¡¡

¡¡

Related Commands

¡¡

APPLy?

¡¡

¡¡

¡¡

¡¡