MEMory Command Subsystem

¡¡

¡¡

The generator has five storage locations in non-volatile memory to store instrument states. The locations are numbered 0 through 4. The generator automatically uses location "0" to hold the state of the instrument at power down. You can also assign a user-defined name to each of the locations (1 through 4) for use from the front panel.
MEMory:NSTates?

MEMory:STATe:DELete¡¡

MEMory:STATe:NAME
MEMory:STATe:RECall:AUTO
MEMory:STATe:VALid?

¡¡

¡¡

¡¡

¡¡

¡¡