FREQuency:SPAN

¡¡

¡¡

Syntax

¡¡

FREQuency:SPAN {<frequency>|MINimum|MAXimum}
FREQuency:SPAN? [MINimum|MAXimum]

¡¡

¡¡

Description

Set the frequency span (used in conjunction with the center frequency) in the Sweep mode and the default unit is Hz.

¡¡

Explanation

¡¡

<frequency> is the frequency value set by the user, MIN selects the minimum frequency span allowed by the specific function and MAX selects the maximum frequency span allowed by the specific function.

¡¡

¡¡

Return Value

¡¡

FREQuency:SPAN? returns the current frequency span.

FREQuency:SPAN? M AX always returns the maximum value of the frequency span.

FREQuency:SPAN? MIN always returns the minimum value of the frequency span.

¡¡

¡¡

Example

¡¡

Set the frequency span to 900Hz: FREQ:SPAN 900

Return Value: 9.000000e+02

¡¡

¡¡

Related Commands

¡¡

FREQuency:CENTer

¡¡

¡¡

¡¡