AM:INTernal:FUNCtion

¡¡

¡¡

Syntax

¡¡

AM:INTernal:FUNCtion {SINusoid|SQUare|RAMP|NRAMp|TRIangle|NOISe|USER}
AM:INTernal:FUNCtion?

¡¡

¡¡

Description

¡¡

Select the shape of the modulating waveform in internal modulation. The modulating waveform can be "SIN", "SQU", "RAMP", "NRAM", "TRI", "NOIS", or "USER" and the default is SIN.

¡¡

¡¡

Explanation

¡¡

To select internal modulation, refer to the AM:SOURce command.

To select carrier waveform function, refer to the FUNCtion command, where {SINusoid|SQUare|RAMP|USER} can be used as the carrier waveform of AM modulation.

¡¡

¡¡

Return Value

¡¡

The query returns SIN, SQU, RAMP, NRAM, TRI, NOIS or USER.

¡¡

¡¡

Example

¡¡

Select arbitrary waveform as the modulating waveform: AM:INT:FUNC USER

Return Value: USER

¡¡

¡¡

Related Commands

¡¡

AM:SOURce

FUNCtion

¡¡

¡¡

¡¡

¡¡