DATA:COPY

¡¡

¡¡

Syntax

¡¡

DATA:COPY <destination arb name>[,VOLATILE]

¡¡

¡¡

Description

¡¡

Copy the waveform from volatile memory to the non-volatile memory with specified name.

¡¡

¡¡

Explanation

¡¡

<destination arb name> may contain up to 12 characters. The first character must be a letter (A-Z or a-z), but the remaining characters can be numbers (0-9) or the underscore character ("_"). Blank spaces are not allowed.
The following built-in waveform names cannot be used with the DATA:COPY command: "EXP_RISE", "EXP_FALL", "NEG_RAMP", "SINC" and "CARDIAC". If you specify one of the built-in waveforms, an error is generated.
Use the DATA:DELete command to delete the waveform in volatile memory or any of the four user-defined waveforms in non-volatile memory.
Use the DATA:CATalog? command to list all waveforms currently stored in volatile and non-volatile memory. The default selection is EXP_RISE.

¡¡

¡¡

Example

¡¡

Copy the VOLATILE waveform into the storage named "ARB1".

DATA:COPY ARB1, VOLATILE

¡¡

¡¡

¡¡

¡¡